levelname=first
numlevelobjs=25

curlevelback=8

curleveltask=0

curlevelmusic=0

<obj0/>
    name=platform2
    rect={-9.51,-3.58,14.49,-5.58}
    drawlayer=1
    rotation=0.000
    endpos={5.49,-4.58}
    invertobj=0
</obj0>


<obj1/>
    name=start
    rect={-7.46,3.85,-3.46,-4.15}
    drawlayer=1
    rotation=0.000
    endpos={5.79,-4.28}
    invertobj=0
</obj1>


<obj2/>
    name=platform2
    rect={-32.36,-3.46,-8.36,-5.46}
    drawlayer=1
    rotation=0.000
    endpos={-17.36,-4.46}
    invertobj=0
</obj2>


<obj3/>
    name=platform2
    rect={12.32,2.58,36.32,0.58}
    drawlayer=1
    rotation=0.000
    endpos={27.32,1.58}
    invertobj=0
</obj3>


<obj4/>
    name=platform2
    rect={13.10,-3.64,37.10,-5.64}
    drawlayer=1
    rotation=0.000
    endpos={28.10,-4.64}
    invertobj=0
</obj4>


<obj5/>
    name=platform2
    rect={-41.00,8.00,-17.00,6.00}
    drawlayer=1
    rotation=0.000
    endpos={-26.00,7.00}
    invertobj=0
</obj5>


<obj6/>
    name=platform2
    rect={35.70,-4.71,59.70,-6.71}
    drawlayer=1
    rotation=0.000
    endpos={50.70,-5.71}
    invertobj=0
</obj6>


<obj7/>
    name=platform2
    rect={56.00,3.00,64.00,1.00}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
</obj7>


<obj8/>
    name=platform2
    rect={33.82,1.54,41.82,-0.46}
    drawlayer=1
    rotation=0.000
    endpos={-1.18,-2.46}
    invertobj=0
</obj8>


<obj9/>
    name=checkpoint
    rect={38.57,9.06,42.57,1.06}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
</obj9>


<obj10/>
    name=bracelet
    rect={-18.00,0.00,-16.00,-2.00}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
    extraparam=2

</obj10>


<obj11/>
    name=platform2
    rect={34.00,10.00,42.00,8.00}
    drawlayer=1
    rotation=0.000
    endpos={-1.00,6.00}
    invertobj=0
</obj11>


<obj12/>
    name=platform2
    rect={34.00,18.00,42.00,16.00}
    drawlayer=1
    rotation=0.000
    endpos={-1.00,14.00}
    invertobj=0
</obj12>


<obj13/>
    name=platform2
    rect={56.00,8.00,64.00,6.00}
    drawlayer=1
    rotation=0.000
    endpos={21.00,4.00}
    invertobj=0
</obj13>


<obj14/>
    name=platform2
    rect={56.00,14.00,64.00,12.00}
    drawlayer=1
    rotation=0.000
    endpos={21.00,10.00}
    invertobj=0
</obj14>


<obj15/>
    name=platform2
    rect={55.00,20.00,63.00,18.00}
    drawlayer=1
    rotation=0.000
    endpos={20.00,16.00}
    invertobj=0
</obj15>


<obj16/>
    name=rigid
    rect={62.00,23.00,71.00,-10.00}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
</obj16>


<obj17/>
    name=rigid
    rect={58.00,-1.00,67.00,-10.00}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
</obj17>


<obj18/>
    name=rigid
    rect={30.00,28.00,37.00,8.00}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
</obj18>


<obj19/>
    name=boss_pig
    rect={45.00,1.00,53.00,-7.00}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
</obj19>


<obj20/>
    name=bird
    rect={24.00,12.00,28.00,8.00}
    drawlayer=1
    rotation=0.000
    endpos={14.00,3.00}
    invertobj=0
</obj20>


<obj21/>
    name=spider2
    rect={-23.00,9.00,-19.00,5.00}
    drawlayer=1
    rotation=0.000
    endpos={-25.00,-1.00}
    invertobj=0
</obj21>


<obj22/>
    name=platform2
    rect={-2.00,2.94,10.00,1.00}
    drawlayer=1
    rotation=0.000
    endpos={13.00,2.00}
    invertobj=0
</obj22>


<obj23/>
    name=mole
    rect={0.83,-1.48,4.83,-5.48}
    drawlayer=1
    rotation=0.000
    endpos={0.00,0.00}
    invertobj=0
</obj23>


<obj24/>
    name=spider2
    rect={-13.72,5.41,-9.72,1.41}
    drawlayer=1
    rotation=0.000
    endpos={-13.69,-0.25}
    invertobj=0
</obj24>




groundlayer0=
[encoded data, 16384 characters]

groundlayer1=
[encoded data, 16384 characters]

groundlayer2=
[encoded data, 16384 characters]

groundlayer3=
[encoded data, 16384 characters]

groundlayer4=
[encoded data, 16384 characters]

groundlayer5=
[encoded data, 16384 characters]



