"The most critical phase of the procedure is undoubtedly the stage of throughout synchronization during the reverse transfer. If the amplitude of the loop falls more than 0.05 %, it can lead to the catastrophic consequences. It is necessary to maintain the stability of the plant power supply by all means."