start timer_xxx = 0
start state_xxx = start

if timer_xxx > 0.001
	(
		start state_xxx = parta
		start model = AACT
		start link_health = AACTtankbay_01	AACTplas1
		start link_health = AACTtankbay_02	AACTplas1
		start link_health = AACTtankbay_03	AACTplas2_01
		start link_health = AACTtankbay_04	AACTplas2_02
		- start link_path = AACTtankbay_01	AACTtankbay_03
		- start link_path = AACTtankbay_03	AACTtankbay_01
		- start link_path = AACTtankbay_02	AACTtankbay_04
		- start link_path = AACTtankbay_04	AACTtankbay_02
		start link_health = AACTturret1_01	AACTplas1
		start link_health = AACTturret1_02	AACTplas2_01
		start link_health = AACTturret1_03	AACTplas2_02
		start emit_rate = AACTtankbay		4.0
		start link_health = AACTwallbit_12	AACTwallbit_11
		start link_health = AACTwallbit_13	AACTwallbit_12
		start link_health = AACTwallbit_14	AACTwallbit_13
		start link_health = AACTwallbit_15	AACTwallbit_14
		start link_health = AACTwallbit_22	AACTwallbit_21
		start link_health = AACTwallbit_23	AACTwallbit_22
		start link_health = AACTwallbit_24	AACTwallbit_23
		start link_health = AACTwallbit_25	AACTwallbit_24
		start link_health = AACTwallbit_26	AACTwallbit_25
		start random = tank P_501 = 1
		start random = tank P_502 = 1
		start random = tank P_503 = 1
		start random = tank P_504 = 1
		start random = tank P_505 = 1
--		start random = tank PW_501 = 1
--		start random = tank PW_502 = 1


	)

if timer_xxx > 10.0
	(
		start emit_rate = AACTturret1		15.0	popup-submergetime	
	)

if timer_xxx > 140.0
	(
		start stage_complete = 100
 	)

