start timer_xxx = 0
start state_xxx = start

if timer_xxx > 0.001
	(
		start state_xxx		= parta
		start player_z		= partb			-85.0	-- tank bays
		start model		= AACT
		start link_health	= AACTtankbay		AACTplas1
		start link_health	= AACTturret1		AACTplas1
		start link_health	= AACTchopperbay	AACTplas1
		start link_health	= AACTrocketpod		AACTplas1
		start emit_rate		= AACTturret1_01	8.0	popup-submergetime
		start emit_rate		= AACTturret1_02	-8.0	popup-submergetime
		start emit_rate		= AACTrocketpod_01	8.0	popup-submergetime
		start emit_rate		= AACTrocketpod_02	8.0	popup-submergetime
		start link_health	= AACTwallbit_12	AACTwallbit_11
		start link_health	= AACTwallbit_13	AACTwallbit_12
		start link_health	= AACTwallbit_14	AACTwallbit_13
		start link_health	= AACTwallbit_15	AACTwallbit_14
		start link_emit_pre	= AACTwallbit_11	AACTchopperbay_01
		start link_emit_pre	= AACTwallbit_12	AACTchopperbay_02
		start link_emit_pre	= AACTwallbit_13	AACTchopperbay_01
		start link_emit_pre	= AACTwallbit_14	AACTchopperbay_02
		start link_emit_pre	= AACTwallbit_15	AACTchopperbay_01
		start link_emit_pre	= AACTwallbit_15	AACTchopperbay_02
		start link_emit_post	= AACTwallbit_11	AACTrocketpod_03
		start link_emit_post	= AACTwallbit_12	AACTrocketpod_04
		start link_emit_post	= AACTwallbit_13	AACTrocketpod_03
		start link_emit_post	= AACTwallbit_14	AACTrocketpod_04
		start link_emit_post	= AACTwallbit_15	AACTrocketpod_03
		start link_emit_post	= AACTwallbit_15	AACTrocketpod_04
	)

if state_xxx = partb
	(
		start emit_rate		= AACTrocketpod_01	6.0	popup-submergetime
		start emit_rate		= AACTrocketpod_02	6.0	popup-submergetime
		start emit_rate		= AACTtankbay		8.0
	)

if timer_xxx > 140.0
	(
		start stage_complete = 100
 	)

