inorganic_stone_soil

Uristocrat: Soil density data from:
http://www.pedosphere.com/resources/bulkdensity/worktable_us.cfm
 
In spite of the weird URL, the site is normal.
 
DF is based on the texture triangle, which you can see here:
http://www.pedosphere.com/resources/bulkdensity/triangle_us.cfm
 
All of these are actually mixes of sand, silt & clay.  Loam is a
roughly equal mix of all three.  So I'll give the percentages of
each that I used to find the density.  For example, SCS = 20/60/20
means that a soil was assumed to contain 20% sand, 60% clay & 20%
silt.  The numbers will always be in the order sand/clay/silt.

[OBJECT:INORGANIC]

[INORGANIC:CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:粘土][DISPLAY_COLOR:7:7:0][TILE:142]
[SOIL]
[SOLID_DENSITY:1210] SCS = 20/60/20
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]

[INORGANIC:SILTY_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:粉质黏土][DISPLAY_COLOR:0:7:1][TILE:142]
[SOIL]
[SOLID_DENSITY:1210] SCS = 5/50/45
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]

[INORGANIC:SANDY_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:砂质黏土][DISPLAY_COLOR:6:7:1][TILE:142]
[SOIL]
[SOLID_DENSITY:1330] SCS = 55/40/5
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]

[INORGANIC:CLAY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:粘壤土][DISPLAY_COLOR:4:7:1][TILE:142]
[SOIL]
[SOLID_DENSITY:1320] SCS = 33/34/33
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]

[INORGANIC:SANDY_CLAY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:砂质粘壤土][DISPLAY_COLOR:4:6:1][TILE:142]
[SOIL][AQUIFER]
[SOLID_DENSITY:1410] SCS = 60/25/15

[INORGANIC:SILTY_CLAY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:粉质粘壤土][DISPLAY_COLOR:7:6:0][TILE:142]
[SOIL][AQUIFER]
[SOLID_DENSITY:1290] SCS = 10/30/60

[INORGANIC:LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:壤土][DISPLAY_COLOR:4:6:0][TILE:142]
[SOIL][AQUIFER]
[SOLID_DENSITY:1410] SCS = 40/20/40

[INORGANIC:SANDY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:砂质壤土][DISPLAY_COLOR:6:4:1][TILE:142]
[SOIL][AQUIFER]
[SOLID_DENSITY:1560] SCS = 65/10/25

[INORGANIC:SILT_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:粉质壤土][DISPLAY_COLOR:0:6:1][TILE:142]
[SOIL][AQUIFER]
[SOLID_DENSITY:1410] SCS = 20/15/65

[INORGANIC:LOAMY_SAND]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:壤质砂土][DISPLAY_COLOR:6:4:0][TILE:141]
[SOIL][AQUIFER]
[SOLID_DENSITY:1690] SCS = 80/5/15

[INORGANIC:SILT]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:淤泥][DISPLAY_COLOR:7:0:1][TILE:142]
[SOIL][AQUIFER]
[SOLID_DENSITY:1450] SCS = 10/10/80

[INORGANIC:SAND_TAN]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:沙][DISPLAY_COLOR:6:4:1][TILE:141]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5

[INORGANIC:SAND_YELLOW]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:黄沙][DISPLAY_COLOR:6:6:1][TILE:141]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5

[INORGANIC:SAND_WHITE]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:白沙][DISPLAY_COLOR:7:7:1][TILE:141]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5

[INORGANIC:SAND_BLACK]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:黑砂][DISPLAY_COLOR:0:0:1][TILE:141]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5

[INORGANIC:SAND_RED]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:红沙][DISPLAY_COLOR:4:4:1][TILE:141]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5

[INORGANIC:PEAT]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:泥炭][DISPLAY_COLOR:2:7:0][TILE:142]
[SOIL][AQUIFER]
[SOLID_DENSITY:850]  Peat was much too high.  This assumes it has some water in it.

[INORGANIC:PELAGIC_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:深海粘土][DISPLAY_COLOR:7:3:1][TILE:141]
[SOIL_OCEAN][AQUIFER]
[SOLID_DENSITY:2200]
Undersea soil densities from "Geotechnical Properties of Deep Continental Margin Soils"
http://www.informaworld.com/index/907178093.pdf

Undersea soils are fairly dense, being compacted.

[INORGANIC:CALCAREOUS_OOZE]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:钙质软泥][DISPLAY_COLOR:3:7:0][TILE:142]
[SOIL_OCEAN][AQUIFER]
[SOLID_DENSITY:2690]

[INORGANIC:SILICEOUS_OOZE]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:硅质软泥][DISPLAY_COLOR:7:7:1][TILE:142]
[SOIL_OCEAN][AQUIFER]
[SOLID_DENSITY:2460]

[INORGANIC:FIRE_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:耐火粘土][DISPLAY_COLOR:6:4:0][TILE:142]
[SOIL]
[SOLID_DENSITY:2300]
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_STONEWARE]