Enemy Engaged RAH66 Comanche Versus Ka52 Hokum - V1.0.1C - 20th March 2000



Manual Changes and Additional Documentation



1. Compatibility With Apache Havoc

You must install Comanche Hokum in to the same root folder as Apache Havoc.

For example:-

C:\Razorworks



2. Menu Screens - Campaign and Mission Planning Screen

The 3D view window on the Campaign and Mission Planning screen can be panned
and zoomed using the pan and zoom keys.



3. In-flight - Basic Handling - Autopilot

The altitude above which the autopilot can be engaged has been lowered from
25 metres to 5 metres (approximately 16 feet).



3. In-flight - Basic Handling - Hover Hold

If 'Novice' avionics is selected then hover hold will engage at any forward
speed.



3. In-flight - Controls - Game

More cheat keys have been added:-

Shift+7    Load air-to-ground weapon package
Shift+8    Load air-to-air weapon package
Shift+9    Load scout weapon package



3. In-flight - Controls - Cockpit Views

Alt+F1     Toggle the HIDSS (Comanche) / HMS (Hokum) display size for a
           sharper (but smaller) display. This only applies to screen
           resolutions greater than 640x480.

Shift+0    Toggle Comanche and Hokum glass cockpits.
           Toggle Apache and Havoc cockpit graphics (Apache Havoc required).
           This key has been added for programmable joysticks.

Three extra instrument views have been included for the Hokum pilot:-

Alt+Delete      Snap to view 1, press again for forward view
Alt+End         Snap to view 2, press again for forward view
Alt+Page Down   Snap to view 3, press again for forward view

These keys have been repeated for programmable joysticks:-

Alt+V           Snap to view 1, press again for forward view
Alt+B           Snap to view 2, press again for forward view
Alt+N           Snap to view 3, press again for forward view



3. In-flight - Missions - Recon

The transmit recon data distance has been increased from 500 metres to one
kilometre.



10. Appendices - Trouble Shooting - Graphics

/nrt       If your 3D card has any difficulty displaying the TADS or EOS MFD
           pages then use the /nrt command line option to disable drawing
           these displays on the virtual cockpit.

           These 3D displays will be visible on the full screen MFD views
           (press F3 and F4 to see these).

/32bit     If your 3D card supports 32-bit rendering then you can enable this
           feature within the game using the /32bit command line option.
