TextBegin
Sturmgeschütz IV, with spaced armor
TextEnd

TextBegin
The StuG IV depicted here is fitted with the longer L/48, 75mm gun and spaced armor skirts. The suspension and the hull's flank are protected with spaced armor.  Spaced armor added some protechtions against normal rounds, but it was specially designed to defeat hollow or shaped charges fired from Bazookas and various other antitank weapons. Up to 80 mm of frontal armor where also added to the front along with Zimmerit  anti-magnetic coating.
TextEnd

TextBegin
4
TextEnd

TextBegin
16-80
TextEnd

TextBegin
75mm-hv
TextEnd

TextBegin
500 m
TextEnd

TextBegin
12AP/10HE
TextEnd

TextBegin
60 kph
TextEnd

TextBegin
155 Km
TextEnd

TextBegin
25 Tons
TextEnd

TextBegin
6/10
TextEnd

TextBegin
6/10
TextEnd

TextBegin
7/10
TextEnd

TextBegin
600
TextEnd